

|  |
| --- |
| MBA5-P22 V8 |
| User guide |

Table of content

[1 Background 3](#_Toc8722561)

[2 Product introduction 4](#_Toc8722562)

[2.1 Introduction 4](#_Toc8722563)

[2.2 Precaution before using battery 5](#_Toc8722564)

[2.3 Charger 5](#_Toc8722565)

[2.4 Notes 6](#_Toc8722566)

[3 Installation instructions 7](#_Toc8722567)

[3.1 Appearance 7](#_Toc8722568)

[3.2 Install Micro SD and SIM cards 7](#_Toc8722569)

[3.3 Battery Charging 7](#_Toc8722570)

[3.4 Buttons and Function Area 8](#_Toc8722571)

[4 Call function 9](#_Toc8722572)

[4.1 Calling numbers 9](#_Toc8722573)

[4.2 Contacts 9](#_Toc8722574)

[4.3 SMS and MMS 9](#_Toc8722575)

[5 Barcode reader-writer 10](#_Toc8722576)

[6 NFC RFID reader 12](#_Toc8722577)

[6.1 Read functionality 12](#_Toc8722578)

[6.2 Write functionality 13](#_Toc8722579)

[7 Other functions 14](#_Toc8722580)

[7.1 Bluetooth 14](#_Toc8722581)

[7.2 GPS 15](#_Toc8722582)

[7.3 Volume setup 16](#_Toc8722583)

[7.4 Sensor 17](#_Toc8722584)

[7.5 Keyboard 18](#_Toc8722585)

[7.6 Network 19](#_Toc8722586)

[7.7 Infrared read-write function (option) 20](#_Toc8722587)

[8 Device characteristics 21](#_Toc8722588)

[8.1 General characteristics 21](#_Toc8722589)

[8.2 User environment 21](#_Toc8722590)

[8.3 Communication 21](#_Toc8722591)

[8.4 Data collection 21](#_Toc8722592)

[8.4.1 Barcode Scanning 21](#_Toc8722593)

[8.4.2 RFID NFC 21](#_Toc8722594)

[8.4.3 Other data modules (option) 22](#_Toc8722595)

[8.5 Developing Environment 22](#_Toc8722596)

[8.6 Accessories 22](#_Toc8722597)

# Background

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Description | Date | Version | Author | Auditor |
| First parution | 14/05/2019 | V1.0 | CLO | ACA |

# Product introduction

## Introduction

The MBA5-P22 V8 PDA is a rugged IP65 mobile terminal designed for use in industrial environments (laundry, construction, logistics, railways, etc.). It runs on the Android 8.1 operating system.

This industrial terminal is available with HF/NFC and/or a 1D/2D scanner. For ease of use, it is supplied with a gun.

The device’s 8000 mAH battery provides long battery duration.

The 5″ FHD touchscreen ensures comfortable reading and can be used with wet hands or gloves.

The rugged terminal also features wireless communication: NFC, 4G/LTE, Wifi, Bluetooth, GPS.

MBA5-P22 can be used with keyboard emulation for 2D scanner to facilitate your software integration.

## Precaution before using battery

* Do not leave battery unused for long time, no matter it is in device or inventory. If battery has been used for 6 months already, it should be check for charging function or it should be disposed correctly.
* The lifespan of Li-ion battery is around 2 to 3 years, it can be circularly charged for 300 to 500 times. (One full battery charge period means completely charged and completely discharged.)
* When Li-ion battery is not in used, it will continue discharge slowly. Therefore, battery charging status should be checked frequently and take reference of the related battery charging information on the manuals.
* Observe and record the information of a new unused and non-fully charged battery. On the basis of operating time of new battery and compare with a battery that has been used for long time. According to product configuration and application program, the operating time of battery would be different.
* Check battery charging status at regular intervals.
* When battery operating time drops below about 80%, charging time will be increased remarkably.
* If a battery is stored or otherwise unused for an extended period, be sure to follow the storage instructions in this document. If you do not follow the instructions, and the battery has no charge remaining when you check it, consider it to be damaged. Do not attempt to recharge it or to use it. Replace it with a new battery.
* Store the battery at temperatures between 5 °C and 20 °C (41 °F and 68 °F)

## Charger

The charger type is GME10D-050200FGu, output voltage/current is 5V DC/2A. The plug considered as disconnect device of adapter.

## Notes

**Note 1:**

Using the incorrect type battery has danger of explosion. Please dispose the used battery according to instructions.

**Note 2:**

Due to the used enclosure material, the product shall only be connected to a USB Interface of version 2.0 or higher. The connection to so called power USB is prohibited.

**Note 3:**

The adapter shall be installed near the equipment and shall be easily accessible.

**Note 4:**

The suitable temperature for the product and accessories is 010℃ to 50℃.

**Note 5:**

CAUTION RISK OF EXPLOSION IF BATTERY IS REPLACED BY AN INCORRECT TYPE. DISPOSE OF USED BATTERIES ACCORDING TO THE INSTRUCTIONS.

# Installation instructions

## Appearance


Une image contenant téléphone mobile, téléphone, équipement électronique, intérieur

Description générée automatiquementUne image contenant intérieur, assis

Description générée automatiquement

## Install Micro SD and SIM cards

The cards sockets are showing as follows:



## Battery Charging

By using USB Type-C contact, the original adaptor should be used for charging the device. Make sure not to use other adaptors to charge the device.

## Buttons and Function Area

1

2

3



4

5

6

7

**Buttons instructions**

|  |  |  |  |
| --- | --- | --- | --- |
| Side button | 1 | Power | Located on left side, press to ON/OFF device. |
| 2 | Function key | Located on left side, its function can be defined by software. |
| 3 | SCAN button | Scanning button located on both sides. There are two scanning buttons. |
| Main button | 4 | Menu | Display main menu. |
| 5 | Home | Touch it back to main screen. |
| 6 | Enter | Press to confirm current selection |
| 7 | Backspace | Return to last step to setup. |

# Call function

## Calling numbers

1. Click icon .

2. Click number key to input phone numbers.

3. Click icon  to call.

4. Click icon  to end call.

## Contacts

1. Click contacts to open contacts list.

2. Click icon  to add new contacts.

3. Click icon  to import/export contacts.

## SMS and MMS

1. Click  to open message window.

2. Click  to input message receiver and contents.


3. Click to send out messages.

4. Click to add attachment pictures and videos.

# Barcode reader-writer

1. In App Center, open 2D barcode scan test.
2. Press “SCAN” button or pull the trigger.

The parameter “Auto interval” can be adjusted.



Caution: Please scan codes in correct way otherwise the scanning will be failed.

1D barcode:



2D barcode:





Max. radiant power: 0.6mW

Wave length: 655nm

IEC 60825-1 (Ed.2.0). 21CFR 1040.10 and 1040.11 standard.

# NFC RFID reader

## Read functionality

1. Click App Center, open “NFC” to read tag information.



1. Place the tag you want to read in front of the RFID antenna as shown below:




1. The tag will be read.

You can also select a text zone to read the tag. It is not needed to open the application since the device is equipped with keyboard emulation.

## Write functionality

The storage of one tag has 4 zones: RESERVED, EPC, TID and USER. Normally, the default password is 00000000. And TID zone can only be read, other zones can be read and written.

1. Click App Center, open “NFC” to write information in the tag.
2. Place the tag in front of the RFID antenna.
3. Write information in the tag by using the keypad as shown below:




# Other functions

## Bluetooth

1. Open “BT Printer” in App Center.

2. In the list of detected devices, click the device that you want to pair.


3. Select printer and click “Print” to start printing contents.



## GPS

1. Click “GPS” in App Center to open GPS test.


2. Setup GPS parameters to access GPS information.



## Volume setup

1. Click “Volume” in App Center.


2. Setup volume by requirements.



## Sensor

1. Click “Sensor” in App Center.


2. Setup the sensor by requirements.



## Keyboard

1. Click “Keyboard” in App Center.


2. Setup and test the main value of the device.



## Network

1. Click “Network” in App Center.


2. Test WIFI/Mobile signal by requirements.



## Infrared read-write function (option)


1. Open infrared function in App Center.

2. Click button “Open” to start infrared scanning function. Click “LED” for infrared scanning aim assist. Depending on different application status to compile different commands to realize infrared read and write function.




# Device characteristics


## General characteristics



## User environment



## Communication



## Data collection


### Barcode Scanning




### RFID NFC




### Other data modules (option)



## Developing Environment



## Accessories

Holster Cradle